Modified web interface from ilya-fedin (4pda.ru)
==================================================
based on the WebUI operator of MTS Russia for Huawei HiLink modems
====================================================================

Tested on the following models: E3272, E3372h, E3372s, E8372, E5372, E5573, E5577.

It should also work with other models on platforms Balong V7R1, Balong V7R2 and Balong V7R11.
For example: E5373 (V7R2), E8278 (V7R1), and so on.


* ADBUpdate_WEBUI_17.100.xx.xx.143_HILINK_Mod1.x_CPIO - universal ADB-broacher
(used as the last instance, when nothing else works, for example, if you have Zong E8372 or Telenor E8372)



* Update_WEBUI_17.100.xx.xx.143_HILINK_Mod1.x_V7R1_V3R2_V3R3.exe
 is the official flasher for the Balong V7R1 (E3272, E3276, E5372)

* Update_WEBUI_17.100.xx.xx.143_HILINK_Mod1.x_V7R2_9x25_V7R11_CPIO.exe
 is the official flasher for the Balong V7R2 and Balong V7R11 (E3372h, E3372s, E8372, E5573, E5577)



* WEBUI_17.100.xx.xx.143_HILINK_Mod1.x_V7R1_V3R2_V3R3.bin
 - firmware file via the web interface for Balong V7R1 (E3272, E3276, E5372)

* WEBUI_17.100.xx.xx.143_HILINK_Mod1.x_BV7R2HS_CPIO.bin
 - firmware file via the web interface for E3372s

* WEBUI_17.100.xx.xx.143_HILINK_Mod1.x_BV7R11HS_CPIO.bin
 - firmware file via the web interface for E3372h


** DO NOT STITCH Balong V7R1 OFFICIAL WASHER OR FILE FILE FROM Balong V7R2 / V7R11 AND VALVE !!!
   Otherwise there will be an error 19! USE ONLY YOUR FILES !!! **